$ EZ-EDS Version 3.25.1.20181218 Generated Electronic Data Sheet

$ Modified by molex
[File]
        DescText = "EthernetIP Scanner/Adapter KRC5";
        CreateDate = 07-11-2011;
        CreateTime = 16:52:29;
        ModDate = 12-07-2020;
        ModTime = 15:12:16;
        Revision = 2.3;
        HomeURL = " ";

[Device]
        VendCode = 121;
        VendName = "KUKA Deutschland GmbH";
        ProdType = 12;
        ProdTypeStr = "Communications Adapter";
        ProdCode = 3;
        MajRev = 5;
        MinRev = 1;
        ProdName = "KR C5 - EtherNet/IP";
        Catalog = "KRC";
        Icon = "Kuka.ico";

[Device Classification]
        Class1 = EtherNetIP;

[Params]
        Param1 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "OT Size",              $ name
                "Bytes",                $ units
                "OT Size",              $ help string
                1,509,256,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param2 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0000,                 $ Descriptor
                0xC7,                   $ Data Type
                2,                      $ Data Size in bytes
                "TO Size",              $ name
                "Bytes",                $ units
                "TO Size",              $ help string
                1,505,256,              $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places
        Param6 =
                0,                      $ reserved, shall equal 0
                ,,                      $ Link Path Size, Link Path
                0x0010,                 $ Descriptor
                0xC8,                   $ Data Type
                4,                      $ Data Size in bytes
                "RPI Adapter",          $ name
                "",                     $ units
                "RPI constrains for Adapter",    $ help string
                4000,5000000,4000,      $ min, max, default data values
                ,,,,                    $ mult, div, base, offset scaling
                ,,,,                    $ mult, div, base, offset links
                ;                       $ decimal places

[Assembly]
        Object_Name = "Assembly Object";
        Object_Class_Code = 0x04;
        Assem1 =
                "OT Data",
                ,
                ,
                0x0001,
                ,,
                4040,;
        Assem2 =
                "TO Data",
                ,
                ,
                0x0001,
                ,,
                4072,;

[Connection Manager]
        Revision = 1;
        Object_Name = "Connection Manager Object";
        Object_Class_Code = 0x06;
        MaxInst = 1;
        Number_Of_Static_Instances = 1;
        Max_Number_Of_Dynamic_Instances = 0;
        Connection1 =
                0x04030002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x66740405,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param6,Param1,Assem1,   $ O->T RPI, size, format
                Param6,Param2,Assem2,   $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,,                      $ target config size, format
                "Local Slave 1 - Exclusive Owner",    $ Connection Name
                "Exclusive owner connection",    $ help string
                "20 04 24 67 2C 66 2C 65";    $ Path
        Connection2 =
                0x04030002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x66740405,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param6,Param1,Assem1,   $ O->T RPI, size, format
                Param6,Param2,Assem2,   $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,,                      $ target config size, format
                "Local Slave 2 - Exclusive Owner",    $ Connection Name
                "Exclusive owner connection",    $ help string
                "20 04 24 71 2C 70 2C 6F";    $ Path
        Connection3 =
                0x04030002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x66740405,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param6,Param1,Assem1,   $ O->T RPI, size, format
                Param6,Param2,Assem2,   $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,,                      $ target config size, format
                "Local Slave 3 - Exclusive Owner",    $ Connection Name
                "Exclusive owner connection",    $ help string
                "20 04 24 7B 2C 7A 2C 79";    $ Path
        Connection4 =
                0x04030002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x66740405,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param6,Param1,Assem1,   $ O->T RPI, size, format
                Param6,Param2,Assem2,   $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,,                      $ target config size, format
                "Local Slave 4 - Exclusive Owner",    $ Connection Name
                "Exclusive owner connection",    $ help string
                "20 04 24 85 2C 84 2C 83";    $ Path
        Connection5 =
                0x04030002,             $ 0-15    = supported transport classes
                                        $ 16      = trigger: cyclic
                                        $ 17      = trigger: change of state
                                        $ 18      = trigger: application
                                        $ 19-23   = trigger: reserved
                                        $ 24      = application type: listen-only
                                        $ 25      = application type: input-only
                                        $ 26      = application type: exclusive-owner
                                        $ 27      = application type: redundant-owner
                                        $ 28-30   = reserved
                                        $ 31      = Direction: Client = 0 / Server = 1
                0x66740405,             $ 0       = O->T fixed size supported
                                        $ 1       = O->T variable size supported
                                        $ 2       = T->O fixed size supported
                                        $ 3       = T->O variable size supported
                                        $ 4-5     = O->T number of bytes per slot (obsolete)
                                        $ 6-7     = T->O number of bytes per slot (obsolete)
                                        $ 8-10    = O->T Real time transfer format
                                        $ 11      = reserved
                                        $ 12-14   = T->O Real time transfer format
                                        $ 15      = reserved
                                        $ 16      = O->T connection type: NULL
                                        $ 17      = O->T connection type: MULTICAST
                                        $ 18      = O->T connection type: POINT2POINT
                                        $ 19      = O->T connection type: reserved
                                        $ 20      = T->O connection type: NULL
                                        $ 21      = T->O connection type: MULTICAST
                                        $ 22      = T->O connection type: POINT2POINT
                                        $ 23      = T->O connection type: reserved
                                        $ 24      = O->T priority: LOW
                                        $ 25      = O->T priority: HIGH
                                        $ 26      = O->T priority: SCHEDULED
                                        $ 27      = O->T priority: reserved
                                        $ 28      = T->O priority: LOW
                                        $ 29      = T->O priority: HIGH
                                        $ 30      = T->O priority: SCHEDULED
                                        $ 31      = T->O priority: reserved
                Param6,Param1,Assem1,   $ O->T RPI, size, format
                Param6,Param2,Assem2,   $ T->O RPI, size, format
                ,,                      $ proxy config size, format
                ,,                      $ target config size, format
                "Local Slave 5 - Exclusive Owner",    $ Connection Name
                "Exclusive owner connection",    $ help string
                "20 04 24 8F 2C 8E 2C 8D";    $ Path

[Capacity]
        TSpec1 = Tx, 505, 1250;
        TSpec2 = Rx, 509, 1250;

[Ethernet Link Class]
        Revision = 4;
        Object_Name = "Ethernet Link Object";
        Object_Class_Code = 0xF6;
        MaxInst = 4;
        Number_Of_Static_Instances = 4;
        Max_Number_Of_Dynamic_Instances = 0;
        InterfaceLabel1 = "XF3";
        InterfaceLabel2 = "XF4";
        InterfaceLabel3 = "XF5";
        InterfaceLabel4 = "XF6";

